!pr0
Avoiding EXTRA DEFINITION ERROR.....................Bill Morgan

No sooner said...

OK, here are some patches to defeat the check for double definitions in the S-C Macro Assemblers.  Just put an RTS ($60) at the appropriate location:

!lm+5
Version 1.0 -- Motherboard: $221D
             Language Card: $E369

Version 1.1 -- Motherboard: $210E
             Language Card: $E228
!lm-5

Be very certain that any double definitions are intentional and identical.  If you use the same label with two different values (unless it's defined with .SE) the assembler cannot produce correct code.
